LEARJET 45 REFERENCE INFORMATION

For detailed instructions on how to fly this aircraft, see the Aircraft Handbook. For standard procedures, see the Checklists tab.

Total Flight Simulator aircraft weight with full fuel
           19,907 lbs

NOTE: To adjust fuel load, on the Aircraft menu, click Fuel.

VMO - Maximum Operating Speed (airspeed)
           330 KIAS (primary display)
           325 KIAS (standby airspeed indicator)

MMO - Maximum Operating Speed (Mach)
            .78 Mach (autopilot disengaged)
            .81 Mach (autopilot engaged)

VA  -  Maneuvering Speed
          12,500 lbs.
                    150 KIAS (sea level)
                    163 KIAS (20,000')
                    195 KIAS (40,000')
          20,200 lbs.
                    198 KIAS  (sea level)
                    225 KIAS (20,000')
                    245 KIAS (40,000')

VLO - Maximum Gear Operating Speed
           200 KIAS

VLE - Maximum Landing Gear Extension Speed
           260 KIAS

VFE - Maximum Flaps Extended Speed
          250 KIAS (flaps 8 degrees)
          200 KIAS (flaps 20 degrees)
          150 KIAS (flaps 40 degrees)

V1 - Takeoff Decision Speed (dry runway; standard temperature)
       107 KIAS (for all conditions, with anti-skid off)

VR - Rotation Speed (dry runway; standard temperature)
        Sea Level
                   108 KIAS (13,000 lbs)
                   118 KIAS ( 20,200 lbs)
        5,000'
                   108 KIAS (13,000 lbs)
                   119 KIAS ( 20,200 lbs)

V2 - Takeoff Safety Speed (dry runway, standard temperature)
        Sea Level
                  120 KIAS (13,000 lbs)
                  129 KIAS (20,200 lbs)
        5,000'
                   120 KIAS (13,000 lbs)
                   130 KIAS ( 20,200 lbs)

VAPP - Approach Climb Speed (flaps 20 degrees; gear up)
             <4,000'
                  106 KIAS (13,000 lbs)
                  127 KIAS (19,200 lbs)
             5,000'
                   107 KIAS (13,000 lbs)
                   128 KIAS ( 19,200 lbs)

VREF - Landing Approach Speed (flaps 40 degrees; gear down)
             <4,000'
                  102 KIAS (13,000 lbs)
                  123 KIAS (19,200 lbs)
             5,000'
                   103 KIAS (13,000 lbs)
                   123 KIAS ( 19,200 lbs)

Best Glide Speed
           160 KIAS (gear and flaps up; both engines inoperative)


NOTE:  For explanations of speeds used on this tab, see "V-speeds" in the Glossary section of Help.