Fokker 100/70 PROCEDURES

Some functions on this checklist are not possible with
The current panel version 5.3
Check Http://Fokker.avsim.net for information and updates
Concerning the upcoming 3D panel which will feature most of
Those functions

____________________________________
BEFORE START

[ ] Seat Belt - No SMKG -- ON
[ ] Fuel Quantity -- CHECKED
[ ] Altimetars -- SET
[ ] Ship's Papers -- ON BOARD
[ ] FMP -- SET
[ ] L-R FMS -- SET
[ ] MFDS/TRP -- SET
[ ] Nav/Com -- SET
[ ] Parking Brake -- SET
[ ] L-R Windows And Doors -- CLOSED

____________________________________
CLEARED FOR ENGINE START

[ ] ENG Anti-Icing -- Check OFF
[ ] Beacon -- ON
[ ] Engine Panel -- SET
[ ] Fuel Pumps -- ON
[ ] Windows And Probe Heat -- ON
[ ] Bleed Press -- CHECK
[ ] Thrust Levers -- FWD IDLE

           -------------
	  |Start Engines|
	   -------------
____________________________________
AFTER START

[ ] Anti-Icing -- SET
[ ] Engine Panel -- CHECKED
[ ] Alert Lights -- OUT
[ ] Flaps -- SET FOR TAKEOFF
[ ] Fuel Levers -- CHECKED OPEN
[ ] Trims -- SET
[ ] Door Selector -- AUTOMATIC

____________________________________
DURING TAXI/BEFORE TAKEOFF

[ ] Flight Instruments -- CHECKED
[ ] FMP -- SET
[ ] ABS -- RTO
[ ] Brake Temperatures -- CHECKED
[ ] TO Data And Breifing -- COMPLETED
[ ] Flight Controls -- CHECKED
[ ] Radar And Transponder -- AS REQUIERD

____________________________________
CLEARED FOR TAKEOFF

[ ] APU -- AS REQUIERD
[ ] TO Config -- CHECKED

____________________________________
TAKEOFF

[ ] Brakes -- RELEASE
[ ] Thrust Levers -- ADVANCE SMOOTHLY TO 40% N1
[ ] Thrust Levers -- ADVANCE SMOOTHLY TO 100% N1
     --or--
     TO/GA Mode -- Engage
[ ] Engine Instruments -- MONITOR
[ ] Airspeed 80 KIAS -- CALLOUT "80 KNOTS"
[ ] Airspeed V1 -- CALLOUT "V1"
[ ] Airspeed VR -- CALLOUT "ROTATE"
[ ] Airspeed V2 -- CALLOUT "V2"
[ ] Landing Gear -- UP (WHEN POSITIVE CLIMB ESTABLISHED)
[ ] Airspeed --MAINTAIN V2+20 KIAS
[ ] Autopilot -- ENGAGE AT 1,000' AGL
[ ] Flaps-- UP AT 210 KIAS
[ ] Autothrottle -- OFF
[ ] Thrust Levers-- 90% N1
[ ] Airspeed -- 250 KIAS AT 3,000' AGL
[ ] Landing Gear Lever -- Verify OFF

____________________________________
AFTER TAKEOFF

[ ] MFDS -- CHECKED
[ ] Altimeters -- SET

____________________________________
CLIMB

[ ] Airspeed -- MAINTAIN 250 KIAS
[ ] Landing Lights -- OFF ABOVE 10,000' MSL
[ ] Airspeed -- 280 KIAS ABOVE 10,000' MSL
[ ] Seat Belt -- OFF ABOVE 10,000' MSL

____________________________________
CRUISE

[ ] Thrust Levers-- AS DESIRED
[ ] Trim -- AS NECESSARY

____________________________________
BEFORE APPROACH/DESCENT

[ ] Seat Belt -- ON BELOW 10,000' MSL
[ ] Landing Alt -- CHECKED
[ ] Ignition -- AS REQUIRED
[ ] ABS -- AS REQUIRED
[ ] MFDS -- CHECKED
[ ] Altimeters -- SET
[ ] Landing Data/Approach Briefing -- COMPLETED
[ ] Airspeed -- <250 KIAS BELOW 10,000' MSL
[ ] Landing Lights -- ON BELOW 10,000' MSL

____________________________________
APPROACH

[ ] Airspeed -- AS DESIRED
[ ] Thrust Levers -- AS DESIRED
[ ] Flaps -- AS DESIRED
[ ] Autopilot -- AS DESIRED

____________________________________
LANDING

[ ] Landing Gear -- DOWN
[ ] Flaps -- SET
[ ] Lift Dampers -- ARMED
     (use Shift+T)

____________________________________
LANDING ROLL

[ ] Thrust Levers -- IDLE
[ ] Autopilot -- CHECK DISENGAGED
[ ] Autothrottle -- CHECK OFF
[ ] Lift Dumpers -- CHECK FULL UP
[ ] Brake -- AS REQUIRED
[ ] Thrust Levers-- REVERSE
[ ] Thrust Levers -- IDLE AT 60 KIAS

____________________________________
TAXI-IN

[ ] Lift Dumpers -- DN
[ ] Flap Lever -- UP
[ ] Pitot Heat -- OFF
[ ] Landing Lights -- AS DESIRED
[ ] Flight Director -- OFF
[ ] Transponder -- AS REQUIRED

____________________________________
PARKING

[ ] Parking Brake -- AS REQUIRED
[ ] Door Selector -- MANUAL
[ ] APU -- AVAILABLE
[ ] Speed Brake And Lift Dumpers -- IN
[ ] Flaps -- SET
[ ] RADAR -- CHECK OFF
[ ] Anti-Icing -- OFF
[ ] Fule Levers -- SHUT
[ ] Flight Controls -- LOCKED
[ ] Seat Belt -- OFF
[ ] Exterior Lights -- CHECK
[ ] Fuel Pumps -- OFF
[ ] Air Conditioning -- SET
[ ] EFIS -- OFF
[ ] MFDS -- CHECKED

____________________________________
FINAL STOP

[ ] APU -- OFF
[ ] BATTERIES -- OFF

____________________________________

NOTE: This aircraft's real-world checklists have been modified for use with Flight Simulator 2002. To learn about using, printing, and customizing checklists, see Help.

Project Fokker 100/70
Http://Fokker.avsim.net